**Q&A**

**Question**: (11) LMR 600 Ultra-Flex cables. Cables are approximately 150’ each.

terminations for each end of the (11) cables. What type of termination do you need for these cables?

**Answer**: Connectors are TNC Male both ends

**Question**: Will you be able to provide any kind of drawings? This will help us determine cable lengths, pathways and quantities.

**Answer**: We are not providing drawings for this project. Room is 80’ x 62’ square, there are multiple walls in the celling that will need penetrations. T-bar ceiling is at 9’, roof is 18’.

**Question**: Is there a need for CAT 6 riser rated PVC or CAT 6 plenum rated?

**Answer**: CAT 6 riser rated

**Question**: Are there minimum ground bus bar lug requirements or grounding to existing ground bus onsite?

**Answer**: There is an existing grounding bus bar located within one of the other rooms inside overall space.

**Question**: What format should final electronic as built be in? AutoCad? If so, will a .dwg file be provided?

**Answer**: Microsoft Visio 2019 drawings

**Question**: What drawings are being referenced?

**Answer**: Drawing will be provided to selected contractor once contract has been awarded.

**Question**: What part number should be used for "Angled Wall Plates"? All other materials have a part number associated with the request.

**Answer**: 41081-2WP - Angled Single-Gang QUICKPORT™ Wallplate, 2-Port, White

**Question**: Will all network drops in Unclassified Horizontal Cabling (ConDev) we surface mounted?

**Answer**: Yes, drops will be surface mounted in single gang white surface mount boxes, 42777-1WA - Surface-Mount Back Box, Single-Gang, 1.89" Box Depth, White.

**Question**: Does the As built need to show drop locations or cabling pathways and Drop locations?

**Answer**: Drop locations, patch panel location and Cable / Port IDs.

**Question**: What type of background checks or requirements are needed for technicians that will be conducting scope? Will this scope require technicians to be escorted within facility?

**Answer**: Contractors will need to be registered in DBIDs for access to Base, escorts will be provided when working in designated spaces.

**Question**: Can floor-plans for each location be provided? If already provided, how can they be accessed?

**Answer**: Floor plans will be provided to selected contractor once contract has been awarded.

**Question**: Can the approx. length of the (16 locations) that require 6F MM OM3 fiber cables be provided?

**Answer**: Approximate length cannot be provided. Room is 80’ x 62’ square, there are multiple walls in the celling that will need penetrations. T-bar ceiling is at 9’, roof is 18’.

**Question**: Can the approx. length of the (2 locations) that require 6F MM OM3 fiber cables be provided?

**Answer**: Approximate length cannot be provided. Room is 80’ x 62’ square, there are multiple walls in the celling that will need penetrations. T-bar ceiling is at 9’, roof is 18’.

**Question**: Can the approx. length of the (16 locations) that require Cat6 UTP cables be provided?

**Answer**: Approximate length cannot be provided. Room is 80’ x 62’ square, there are multiple walls in the celling that will need penetrations. T-bar ceiling is at 9’, roof is 18’.